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2-Motor and 3-Motor Height Adjustable Tables – (“HATs”)

(Empire series and V-Flex series)
Programming the remote control              [image: ]


1. Default settings – Max and Min height

When the HATs are first set up, the remote is pre-programmed to stop at a maximum height of 1,283 mm (48 3/4”) and a minimum height of 597 mm (23 ½”).

2. Changing the max and min range

Raise or lower the HAT to a comfortable height with the up and down buttons (the arrows “[image: ]” or ” [image: ]”), so that you can see the remote clearly.

Press the M button for about 3-5 seconds until you see ‘S---1’ on the remote display.

Release the M button and then press it again, and a code ‘1Un’ will appear.

Press either the up or down arrow buttons a few times. You will cycle through several codes. When you see the code ‘7SH’ stop and press the M button again. You will see a code “[image: ]’. If you press one of the arrow buttons again, the code will change to either:

[image: ]   or   [image: ]

	[image: ]   is to set the lowest height

After you see the  [image: ] code, push the M button once, and you will see the current lowest height. If this is the first time you are changing this setting, then you should see the default lowest height = 23 ½”. When you see that, you can push the up arrow button multiple times, which will increase the number you see incrementally by .04” per push. 

When you see the height you want the HAT remote to memorize, press the M button once.




The new lowest height will now be memorized, and you can test the HAT after a few seconds to see if you have been successful.


   	[image: ]	 is to set the highest height

The same procedure applies if you want to change the highest height, except after you see the [image: ] code, press the up or down arrow once or twice until you see  [image: ]. Then follow as above for the lowest height setting. 

You should first see the last highest height setting, and then you push the down arrow button several times until you see the height you want the HAT remote to memorize. Then press the M button once. 

The new highest height will now be memorized, and you can test the HAT after a few seconds to see if you have been successful.
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